Thank you for purchasing an EPSON serial impact dot matrix printer. 
This README file contains the latest information about your EPSON product.
                                                          2/18/2002
---------------------------------------------------------------------

Using device fonts with Microsoft Office 97
===========================================

You may have problems printing using device fonts with Microsoft Office 97.
If this occurs, change the following setting:

*Change the compatibility mode from Office 97 to Office 95.


Notes for EPSON Status Monitor
==============================

1. General troubleshooting solutions

1-1. If a Windows shared printer cannot be monitored, check the following:

	*Make sure that the printer driver is installed on the computer
	 that is hosting the Windows shared printer and that, in the printer
	 driver, the printer is set to be shared. Also make sure that "Allow
	 monitoring of shared printers" is selected in the Monitoring 
	 Preferences dialog box.

	*(Windows Me/98/95) On the server, double-click the Network icon in
	 Control Panel and make sure that the "File and printer sharing for
	 Microsoft Networks" component is installed. Then, on the server AND
	 clients, make sure that the "IPX/SPX-compatible Protocol" or the
	 "TCP/IP Protocol" is installed.

	*On the server and clients, make sure that Printer Interface version
	 4.xxx or later is installed. To confirm the version of Printer
	 Interface, open the EPSON Status Monitor 3 dialog box and click the
	 icon on the left side of the EPSON Status Monitor 3 title bar. Select
	 "About..." from the menu and confirm the version in the "Aboutc"
	 message box that appears.

1-2. Limitation when monitoring network printers in a Windows 95 environment

Windows Socket 2 must be installed. Windows Socket 2 is available from 
Microsoft Corporation.

1-3. If network printers cannot be monitored after returning from sleep mode in  a Windows 95 environment, do the following:

Close the printer driver and EPSON Status Monitor 3, then restart the Status Monitor. For information on accessing the Status Monitor, see your printer's Reference Guide.


2. Solutions for Windows XP/2000/NT environment

2-1. When uninstalling EPSON Status Monitor 3 from a multi-user Windows 
XP/2000/NT environment, remove the shortcut icon from all clients before 
uninstalling. You can remove the icon by clearing the Shortcut Icon check
box in the Monitoring Preferences dialog box.

2-2. The EPSON Status Monitor 3 utility is not available when printing from 
a Remote Desktop connection.


3. Solutions for network printers

3-1. To monitor a NetWare printer, connect only one print server to each
queue. For directions, see the Administrator's Guide for the printer.

3-2. You cannot monitor a NetWare queue printer beyond the IPX router
because the setting for IPX hops is 0.

3-3. When monitoring NetWare printers, a Novell Client that corresponds
to your operating system must be used. Operation is confirmed for the
versions below.

	*For Windows Me/98/95: Novell Client 3.31 for Windows 95/98
	*For Windows 2000/NT 4.0: Novell Client 4.81 for Windows NT/2000

3-4. Limitation when monitoring NetWare printers

This product supports NetWare printers configured by a queue-based printing
system such as Bindery or NDS.  You cannot monitor NDPS (Novell Distributed
Print Services) printers.


4. Solutions for using EPSON Status Monitor 3 for impact printers.

4-1. Notes on error and warning notification when printing

    *If connecting to a NetWare printer and monitoring it while printing, make
     sure EPSON Status Monitor 3 is running.

    *If connecting to an LPR printer and monitoring it while printing, make
     sure EPSON Status Monitor 3 is running.

    *When connecting to a Windows 2000/NT shared printer from Windows Me/98/95, error and
     warning notifications do not appear during printing. Make sure EPSON Status
     Monitor 3 is running, and use the Printer Status Window to find out about errors.

    *When connecting to a Windows XP shared printer, error and warning notifications do not appear during printing. Make sure EPSON Status Monitor 3 is running, and use the Printer Status Window to find out about errors.

    *When connecting to a shared printer beyond a router, error and warning notification for shared printers during printing is not available in some cases because of the router's settings.


---------------------------------------------------------------------
General notice: Product names used herein are for identification 
purposes only and may be trademarks of their respective owners. 
EPSON disclaims any and all rights in those marks.

(C)SEIKO EPSON CORPORATION 2002

END
